香港九龍啟成街3號[image: image1.jpg]BIi2E
EMSD




3 Kai Shing Street, Kowloon, Hong Kong

電 話 Tel: (852) 3912 0642
傳 真 Fax: (852) 2890 6081

電 郵 Email: dcs@emsd.gov.hk

網 址 Website: www.emsd.gov.hk

Application Form for District Cooling Services
For Government Users
	To:  The Director of Electrical & Mechanical Services

This B/D hereby apply for the following (Please tick in the appropriate box):



	(
	New Application for Approval as the Approved Consumer for a Building
	(          
	Revision of Contract Cooling Capacity

	Account No. (if any)
	
	*Intended Services Starting Date/ Effective Date
	
	/
	
	/
	
	

	
	
	
	Day
	
	Month
	
	Year
	

	Applicant/Approved Consumer Information



	Bureau / Department 
Name of Responsible Officer
Designation
Rank
Tel. No.
Fax No.
Email
Service Address

Service Address Tel. No.



	Details

	
	
	
	
	
	

	Estimated Maximum Cooling Capacity/

Proposed Revised Contract Cooling Capacity*

	
	kWr 
	
	
	

	
	                
	
	
	
	

	Request for an additional smaller heat exchanger

	(
	Yes
Capacity:            kWr 

	(
	·  No

	Remarks:

· Please submit a detailed cooling load calculation to support the above figures.

	UNDERTAKING
This B/D undertakes-
1. to be responsible, including funding, for the design, provision, construction, installation and maintenance of the facilities for the building to receive district cooling services as specified by the Director of Electrical and Mechanical Services;
2. to comply with the District Cooling Services Supply Conditions and the Technical Guidelines for Connection to District Cooling System as revised by the Electrical and Mechanical Services Department from time to time; and
3. to ensure all installations (except heat exchanger and primary chilled water pipe) installed inside the substation of the concerned building is designed, installed, inspected and tested in accordance with all the requirements of the District Cooling Services Ordinance, Chapter 624 and the Technical Guidelines for Connection to District Cooling System.
4. to share the utility costs arising from the provision of district cooling services for the building by allocation warrants to the EMSD and such costs will be calculated by the EMSD based on the estimated/ actual cooling consumption.
Name of B / D 
Name Responsible Officer
Designation:
Rank:
Signature
Date:


	


Notes to Applicant/Approved Consumer
1. For "Revision of Contract Cooling Capacity" application that proposes to increase the contract cooling capacity, it is subject to the availability of capacity from the system network and physical size of substation and thus it cannot be guaranteed.  The application for reduction of contract cooling capacity may only be allowed after one year of continuous district cooling services subscription at the current contract cooling capacity for the related building.
2. Time to provide district cooling services connection will depend on the location of the building under application and the required cooling capacity.
3. Minimum chilled water flow rate at consumer side of each heat exchanger is 20% of its nominal flow rate.  If the applicant estimates that the cooling demand for district cooling services is often very low comparing to the estimated maximum cooling capacity, an additional smaller heat exchanger may be requested to cater the low load conditions.  The applicant should provide relevant information for EMSD’s consideration and approval.  Larger size of substation for installation of additional heat exchangers should be provided by the applicant.

	* Delete as appropriate 删除不適用者      機 電 工 程 署 Electrical and Mechanical Services Department 
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